**Major VT 8 Test Procedure Errors:**

1. **Correctly identify the vehicle and record the test on the MOT Testing Service system.**
2. **No Interior checks done**
3. **No Exterior checks done including one or all of the following:-**
4. Front of vehicle not checked
5. Offside of vehicle not checked
6. Rear of vehicle not checked
7. Nearside of vehicle not checked

1. **Headlight aim & use of headlamp aim equipment**
2. Headlamp aim tester not used to assess headlamp aim.
3. **No Under bonnet checks done**
4. **Jacking of vehicle – front, use of turntables**.
5. Front of vehicle not jacked
6. **Jacking of vehicle – (¹ rear)**
7. Rear of vehicle not jacked
8. **Use of equipment – Brake Tests**
9. Did not carry out the brake test using the appropriate test using the appropriate, approved, brake test equipment.
10. **Performance Checks – Brake Tests**

1. Did not carry out a Service Brake test.
2. Did not carry out a test on front service brakes.
3. Did not carry out a test on rear service brakes.
4. Did not carry out a test on the parking brake.
5. **Use of Equipment. Emission Procedure.**
6. No Emissions test carried out using the appropriate, approved equipment.
7. Did not carry out an appropriate emissions test eg Cat test of none cat vehicle.
8. Incorrect limits used.
9. **Incorrect assessment of testable items incorrect decision**

All other checks omitted from a tester’s inspection are rated as Minor Errors / omissions.

Each Inspection manual section has a maximum total of minors allowed which when exceeded results as a Major error and result in the tester/candidate failing the demonstration test.